Keywords: mud pump，rotary table,swivel,hook,crown block ,bearing,drilling rig bearing

3NB 500C typeMud pump bearing:：

drive bearing

Current model of cylindrical roller bearing: NU3036X2M/C9 original model: 32836HU connecting rod large head bearing

Current model of cylindrical roller bearing: NFP38/600X2Q4 original model: 228/600Q

Connecting rod small head with bearing double row long cylindrical roller bearing: NNAL635Q4/C9W33X original model: 354935QU

The spindle bearing roller bearing is the original type: 24056CA/W33 type: 4053156H

3NB 800 type Mud pump bearing::

Connecting rod large head bearing cylindrical roller bearings: NFP38/600X2Q4 original model: 228/600Q

Connecting rod small head with bearing double row long cylindrical roller bearing: NNAL635Q4/C9W33X original model: 354935QU

Main shaft bearing double row tapered roller bearings: 352960X2 original model: 97860 drive bearing

The spherical roller bearing type: 23136/W33 original model: 3003736

F 1000 type Mud pump bearing::

Drive bearing

Current model of cylindrical roller bearing: NU3040X3M/C9 original model: 32840HU

Connecting rod large head bearing cylindrical roller bearings: NUP4647744Q4/C9 original model: 929/558.8QU

Connecting rod small head with bearing double row long cylindrical roller bearing: NNAL6/177.8-2Q4/C9W33XYA2 original model: 254936QU

The spindle bearing roller bearing is the original type: 24056CA/W33 type: 4053156H

3NB 1000C Mud pump bearing::

Drive bearing

Current model of cylindrical roller bearing: NU3040X3M original model: 32840H

Connecting rod large head bearing cylindrical roller bearings: NFP38/630Q4 original model: 30228/630Q

Connecting rod small head with bearing double row long cylindrical roller bearing: NNAL6034X2M/C9W33X original model: 154734HU

The spindle bearing roller bearing type: 24064CA/W33YA2

3NB 1000 type Mud pump bearing::

Connecting rod large head bearing cylindrical roller bearings: NFP38/630Q4 original model: 30228/630Q

Bearing long cylindrical roller bearings for connecting rod small heads: NAL4034M/C9 original model: 4104134H

Double row tapered roller bearing of spindle bearing: 352064X2 original model: 2097164

Drive bearing is the original spherical roller bearing type: 23140/W33 type: 3003740Y

SL3NB 1300 type Mud pump bearing::

Connecting rod large head bearing cylindrical roller bearings: NUQ19/710/C9W33 original model: 10929/710U

Drive bearing cylindrical roller bearing current model: NU2344M/C9YA4 original model: 32644HU

Present model of bearing cylindrical roller bearing for connecting rod small head: NU2322EM/C9 original model: 32622HU

The spindle bearing roller bearing is the original type: 23160/C9W33 type: 3003760UY

F 1300 type Mud pump bearing::

Drive bearing

Current model of cylindrical roller bearing: NU3044X3M/C9-1 original model: 32844HUI

Connecting rod large head bearing cylindrical roller bearings: NUP464776Q4/C9YA4 original model: 928/660.4QU

Connecting rod small head with bearing double row long cylindrical roller bearing: NNAL6/206.375Q4/W333XYAZ original model: 254941QU

The spindle bearing roller bearing is the original type: 24060CA/C9W33 type: 4053160HU

3NB1300C type Mud pump bearing::

Drive bearing cylindrical roller bearing current model: NU3044X3M/C9-1 original model: 32844HU1

Connecting rod large head bearing cylindrical roller bearings: NFP38/666.75X3Q4 original model: 228/666.75Q

Connecting rod small head with bearing double row long cylindrical roller bearing: NNAL6036X2-2M/W33X original model: 154836H

The spindle bearing roller bearing is the original type: 24072CA/W33 type: 4053172H

3NB1300 type mud pump type Mud pump bearing::

Connecting rod large head bearing cylindrical roller bearings: NFP38/666.75X3Q4 original model: 228/666.75Q

Connecting rod small head with bearing double row long cylindrical roller bearing: NAL4036M/C9 original model: 4104136HU

The present model of double row tapered roller bearing of spindle bearing: 252072X2/C9 original model: 2097172U

Drive bearing is the original spherical roller bearing type: 23144CA/W33 type: 3003744Y

SL3NB 1600 type Mud pump bearing::

Drive bearing cylindrical roller bearing current model: NU232EM/C9 original model: NU2344M/C9YA4

Connecting rod large head bearing cylindrical roller bearings: NUP6/840/C9 original model: 929/840U

The bearings of the ZP 375 type turntable are as follows:

Main shaft bearing double row thrust angle contact ball bearing: 2327/1049YA original model: 2687/1049

Drive bearing is the original spherical roller bearing model: 22330 type: 3630H

Drive bearing cylindrical roller bearing current model: NU2330EM original model: 32630H

The bearings of the ZP 275 type turntable are as follows:

The present model of the thrust angle contact ball bearing of the spindle bearing: 5692/800 original model: 91682/800

Positive bearing thrust angle contact ball bearings: 5611/800 original model: 1681/800

Drive bearing cylindrical roller bearing current model: NU2330EM original model: 32630H

Drive bearing is the original spherical roller bearing model: 22330 type: 3630H

The bearings of the ZP 205 type turntable are as follows:

The present model of the thrust bearing contact ball bearing bearing of the spindle bearing: 5692/650X1/YA3 original model: 1687/650

Bearing type bearing thrust angle contact ball bearing bearing type: 5617/620 original model: 1687/620

Drive bearing cylindrical roller bearing current model: NU2330EM original model: 32630EH

Drive bearing is the original spherical roller bearing model: 22330 type: 3630H

The bearing of the hook is as follows:

The current model of the thrust cylindrical roller bearing of the spindle bearing: 89468M original model: 9889468

The present model of the thrust cylindrical roller bearing of the spindle bearing: 81436X3/YA original model: 549836K

The present model of the thrust cylindrical roller bearing of the spindle bearing: 87436ZW original model: 7549436H

Main type of thrust ball bearing of spindle bearing: 51260M original model: 8260H

The bearings contained in the faucet are as follows:

The present model of the thrust roller bearing of the spindle bearing: 99440Q4 original model: 9019440

The current model of the thrust roller bearing of the spindle bearing: 99456Q4 original model: 9019456Q

Main type of thrust roller bearing of spindle bearing: 91754Q4 original model: 19954EQ original model: 37941K

TC315 type

The present model of double row tapered roller bearing of spindle bearing: 352952SX2/YA original model: 2097952K

TC450 type

The present model of double row tapered roller bearing of spindle bearing: L357049NW-L357010CD2 original model: 37961K

The bearings of the ZP175 type turntable are as follows:

Current model of thrust bearing angle contact ball bearing with positive bearing bearing: 5617/520 original model: 1689/520

The present model of the thrust angle contact ball bearing of the spindle bearing: 5692/530 original model: 91682/530

Drive bearing cylindrical roller bearing current model: NU2322EM original model: 32622H

Drive bearing is the original spherical roller bearing type: 22322CA/W33 type: 53622H